Prebuilt waterproof:

Bang good waterproof servo = 972.43 (6.8k for 7)

Waterproofing manually (quite durable):

Method 1:

Materials reqd. :

Marine grease (730 Rs. For 7)

Plasti dip(900 Rs. For 7) (amazon)

Procedure:

Use marine grease on the top side of the servo where the gear is present, ehich does not allow water to flow from the top side of the servo.

Then use plasti dip to coat the servo with the plastic material which acts like a shrink tape when it dries and makes it really waterproof

During the plasti dip process we need to be careful to remove any air pockets near the edges during the drying phase and also make sure that the servo rotates in the drying phase

Once the plasti dip dries it looks like that there is an layer of plastic coat all over the servo which looks really sturdy